WISE  HOPS
Flexible Steel Wire Ropes  fGalvanised)

Flexible Steel Wire Rope.
6 Strands, each 12 Wires 	Extra Flexible
Steei Wire Rope
6 Strands,
^ach 24 Wires 	Special Extra
Flexible Steel \Vire Rope 	

	6 Strands, eacn
37 \\.res 	Special Make 	
|
5 	o 	! 	|jl_ 	| 	| 	j 		0> 	£ 	
5 	&« g 	55 	~"2 * a- 	~  X 	cc 	u o 	1     i   s 	£> 	
S 		tfl 			fee 			2 	
CS
1 	"Si
1 	Brenkin 	JJ-S rf 	1 	1 	~* a» 	1        1
i      *"* 	|
1
d5 	
Inches. 	Lbs. 	Tons 	Inches 	Lhs 	Tons          Lba. 	"
Tors 	Toi.b 	Inches 	
1 	63 	1 75 	6 	•SS 	J 93         10          — 	— 	1 	
14 	1 06 	2 5 	74 	1 31 	4 45 	1 56        — 	— 	1^ 	
	1 44 	40 	9 	1 S8 	6-7 	2«>          725 	— 	H    ' 	
If 	2-0 	5-5 	10^ 	25 	8'7o 	288 	100 	— 	l| 	
2 	244 	7 0 	1'2~ 	3*5 	11 85 	40 	130 	— 	2 	
2£ 	337      90 	134 	4 5 	14 6 	488       1575       — 	2i    ' 	
24 	4 59 	120 	15 	5 44 	18 55 	5S8 	19 75 	— 	24 ; 	
23 	5 *23 	150 	164 	623 	21 95 	7 0 	240 	— 	•Jf 	
3 	625 	1*0 	18 	7'63 	2.5-7 	82o 	•290 		 	3 	
3£ 	7<»6 	2-2-0 	194 	9*37 	308 	10 3S 	3^ 5 		 	3i 	
54 	S2o 	260 		10-75 	35-2 	11 5 	385 	— 		
	987 	290 	224 	12-19 	41 1 	13 •.•?*< 	445 	— 	3| 	
4 	11-23 	3*0 	24 	1362 	4t>-3 	15 '25 	51-0 		 	4 	
4| 	12.^5 	360 	254 	15-69 	52-9 	17 12 	580 		 	4^ 	
*4 	1344 	390 	27 	1775 	586 	190 	63 5 	— 	4k 	
	— 	— 	— 	1988 	66*4 	21 -69 	71 25 	— 	4| 	
5* 	— 	— 	— 	22 5 	742 	2*38 	79 25 	— 	5 	
54 	— 	— 	— 	2325 	82 -sg 	2769 	S7'75 	— 	54 	
51 	— 	— 	— 	24*5 	91 55 	31-0 	96-75 	— 	54 	
	— 	— 	_— . 	— 	— 	3375 	10V75 	— 	5J 	
6* 	— 		 		 	— 		 	365 	113-75 	— 	6 	
64 	— 		 		 		 		 	425 	132 0 		 	«4 	
7 	— 	— 	— 	— 	— 	485 	154-0 	— 	7 	
n 	— 	— 	— 	— 	— 	550 	17^-5 	— 	74 	
8 	— 	— 	— 	— 	— 	630 	19S-0 	202 	S 	
9 		 	— 	— _ 	— 	— 	79-0 	250-0 	257 	9 	
10 	— 		 	— 	_ 	_ 	980 	305-0 	31S 	10 	
11 		 		 		 	— . 	— 	120-0 	— 	381 	11 	
12 	— 	— 	— 	— • 	— 	142-0 	— 	455 	12 	
In these Flexible Wire Rope Tables, which have been prepared by Messrs. Bolhvant & Co,
Ltd, (who guarantee the above figures as regards new ropes supplied by them)t the wire Is
calculated as taking a breakmar stress of 90 tans to the square inch ; ropes made of wi» which 11
calculated above that will take a proportionately higher breaking: stress